**Machine learning methods for better water quality prediction (79 Citations) 2019**

Ahmed, A. N., Othman, F. B., Afan, H. A., Ibrahim, R. K., Fai, C. M., Hossain, M. S., ... & Elshafie, A. (2019). Machine learning methods for better water quality prediction. *Journal of Hydrology*, *578*, 124084.

Water quality parameters are of considerable significance in any aquatic system analysis.

Traditional modelling methodologies involve large amount of unknown datasets and is a time-consuming process.

AI can identify non-linear and complex relationships.

Johor river basin major degradation because of developmental and human activities

Water Quality prediction model for better water resource management is of critical importance.

Adaptive Neuro-Fuzzy Inference System (ANFIS), Radial Basis Function Neural Networks (RBF-ANN), and Multi-Layer Perceptron Neural Networks (MLP-ANN) were studied with historical data of water quality parameters. WQ parameters of focus were Ammoniacal Nitrogen (AN), suspended solid (SS) and pH. There were twelve input parameters and data from 2009-2010 were used.

This study also assesses significance of every input parameter partitioning NN’s connection weight and also assesses most effectual input using a single and a combination of parameters.

(Wavelet de-noising technique) WDT-ANFIS outperformed other models with R^2 greater than or equal to 0.9 in predicting both pH and SS. Model could also capture temporal patterns in WQ

**Predicting Urban Water Quality with Ubiquitous Data (39 citations) 2016**

Liu, Y., Liang, Y., Liu, S., Rosenblum, D. S., & Zheng, Y. (2016). Predicting urban water quality with ubiquitous data. *arXiv preprint arXiv:1610.09462*.

Novel data-driven approach to forecast WQ by fusing multiple sources of urban data

Urban water quality is of great importance to our daily lives and prediction of wq is important to control water pollution and human health.

Water quality in urban spaces vary non-linearly and depend on multiple factors such as meteorology, water usage patterns and land uses.  
This study forecasts WQ from monitoring stations from WQ data and water hydraulic data by implementing a data-driven approach. It also fuses multiple datasets from different domains into a unified learning model

**Participatory research to monitor lakewater pollution 2021 (0 )**

Aronoff, R., Dussuet, A., Erismann, R., Erismann, S., Patiny, L., & Vivar‐Rios, C. (2021). Participatory research to monitor lake water pollution. *Ecological Solutions and Evidence*, *2*(3), e12094.

Used E.coli bioindicator for detecting raw sewage contamination. Results found microbial burdens occurred during music festivals

Contamination of lake water causes human health issues in lakes used for recreational activities like swimming. Monitoring water quality is crucial (through microbial abundance) to avoid risks to health along shoreline recreational areas

Study confirms Power of participatory research: dedicated people on a budget can do meaningful environmental monitoring.  
  
Open science can bridge academic, public(governmental) and commercial worlds. Partocopatory research and community science are more preferable over

Each site was tested for pH, temp, DO and turbidity

\*\*Algal blooms producing toxins or depleting oxygen

**Continuous Monitoring of Water Quality Using Portable and Low-Cost Approaches (49 citations) 2013**

Tuna, G., Arkoc, O., & Gulez, K. (2013). Continuous monitoring of water quality using portable and low-cost approaches. *International Journal of Distributed Sensor Networks*, *9*(6), 249598.

Measuring water quality at drinking water reservoir require collecting large number of samples.  
Wireless sensor network based monitoring system was used for monitoring

WQ is one of the main factors to control health and state of disease in people and animals.

Anthropogenic inputs such as industrial and municipal wastewater discharge largely determine surface WQ.  
Lakes and rivers are main drinking water sources

Sustainable use of water quality resources require surface water assessment monitoring prigrams.

Water Framework Directive(WFD), major reference to guide efforts to attain sustainable aquatic environment consitsts of guidelines defining the categories f parameters required: DO, pH, EC, temp, turb and nitrate are main params to determine WQ as stated by WFD 7 US EPA

Main problem in surface WQ monitoring is complexity associated with collecting LARGE number of samples.

Fixed monitoring systems require high initial start-up cost but provide real-time data.  
Portable devices does not provide real-time WQ data

**Youtube Videos**

Cyanobacteria/blue-green algae -> find what is in the lake   
Oxygen in the atmosphere from Great Oxygenation Event, about a couple of billion years ago, was created by cyanobacteria. Cyanobacteria -> microalgae . Seaweed- macro algae

Toxic algae kills marine animals and harmful to human health. They grow in warm temperature, need plenty of light and nutrients. Calm waters. Nutrients act like fertilizers (just like plants) Blooms are usually because of human’s effect on the ecology  
Nutrient sources that cause the blooms are varied so hard to pin point exactly which nutrient is causing the bloom (is it agricultural/septic systems that are not controlled well, is it runoff from lawn/grass fertilizers. Pinpointing exact trigger is difficult

HAB (Harmful Algal blooms)

Algal blooms can be seen near shoreline. Some are harmless but others can release toxins that are harmful for people and animals. Algal blooms prevent the use of water resources either for drinking or for other purposes/ recreation

**Water Quality Characterization of Varsity Lake, University of Malaya, Kuala Lumpur, Malaysia 2010 (39)**

Ashraf, M. A., Maah, M. J., & Yusoff, I. (2010). Water quality characterization of varsity lake, University of Malaya, Kuala Lumpur, Malaysia. *E-Journal of Chemistry*, *7*(S1), S245-S254.

Increased levels of nitrogen in the water, combined with phosphorus, can cause excessive plant and algal growth that depletes oxygen levels, possibly to lethal levels.

Some algal blooms also produce toxins that can affect aquatic life or humans that consume them

**Eco-Heart Index as a tool for community-based water quality monitoring and assessment 2018 (11)**

Sakai, N., Mohamad, Z. F., Nasaruddin, A., Abd Kadir, S. N., Salleh, M. S. A. M., & Sulaiman, A. H. (2018). Eco-Heart Index as a tool for community-based water quality monitoring and assessment. *Ecological Indicators*, *91*, 38-46.

The collection of hydrological data often requires advanced technology and a high cost,

This study uses 6 water quality parameters: pH, heavy metals, chemical oxygen demand(?), transparency, ammonia nitrogen and dissolved oxygen.

Water quality monitoring was done using Pact Test and LAQUAtwin. Pact test for pH, COD, NH3-N and heavy metals. works by colorizing a specific parameter by dipping a plastic tube containing a coloring agent into a sample to quantify its concentration by comparison with a color indicator.

LAQUAtwin is a handheld meter that can check a water quality parameter within a minute by simply dipping its sensor into a sample.

community-based monitoring enabling the community to participate in citizen science.

A transparency tube was used for the analysis of turbidity. It can be easily prepared with a transparent tubing and a secchi disk attached to its bottom. The transparency is recorded by a maximum height of a water sample poured into the tubing where the secchi disk is visible from the top. **Although the result is more or less affected by observers**, and the measurement range is generally narrower than a turbidity meter, this method is much simpler and more economical than those used in turbidity and TSS.

A portable DO meter was used for the DO measurement. Although it incurs a high initial cost, proper usage and maintenance allows for accurate and long-lasting measurements with minimal maintenance cost.

The eco-heart index is strongly correlated with WQI and is more informative and attractive to drive policies.

Langat River basin in Malaysia- pollution detected in mid-stream and downstream areas, particularly in populated and land development areas

Malaysia is no exception and water pollution is one of the most serious water resource management

issues in the country. According to the Department of Environment Malaysia (DOE), 36.6% of rivers in Malaysia were classified as slightly polluted, and 5.2% of rivers were classified as

polluted

[**A Study on Water Quality Status of Varsity Lake and Pantai River, Anak Air Batu River in UM Kuala Lumpur, Malaysia and Classify it based on (WQI) Malaysia**](https://eqa.unibo.it/article/view/7967) **2018 (1)**

GAFRI, H. G. F. (2018). A Study on Water Quality Status of Varsity Lake and Pantai River, Anak Air Batu River in UM Kuala Lumpur, Malaysia and Classify it based on (WQI) Malaysia. *EQA-International Journal of Environmental Quality*, *29*, 51-65.

turbidity, nutrient, nitrate, ammonia, and phosphate DO, COD, SS, BOD, NH3-N, and PH, *E.coli* and Total *Coliform*

The agro-industry, which consumes 70% of the water resources in Malaysia, severely pollutes the rivers from point sources and non-point sources.

According to Department of Environment Malaysia (DOE, 2012), there are three parameters of contamination that significantly affect river quality; BOD, SS, and NH3-N (Ammoniacal Nitrogen).

**Automated Water Quality Survey and Evaluation Using an IoT Platform with Mobile Sensor Nodes 2017 (31)**

IoT platform measured Temp, pH, DO, EC, ORP. The developed platform provided a cost-effective, fast, deployable, and easily maintainable solution for the high-resolution ~~spatiotemporal~~ telemoitoring of surface water.

The data collected in this approach can benefit aquatic environmental monitoring in various applications such as the survey of an unknown area for collecting useful knowledge to establish an environmental model, the design of a sensor deployment strategy for long-duration monitoring, an analysis of microaquatic environmental changes, and so on.

### [Autonomous in situ measurements of noncontaminant water quality indicators and sample collection with a UAV](https://www.mdpi.com/433254) 2019 (12)

Koparan, C., Koc, A. B., Privette, C. V., & Sawyer, C. B. (2019). Autonomous in situ measurements of noncontaminant water quality indicators and sample collection with a UAV. *Water*, *11*(3), 604.

UAV assisted autonomous water sampling system (UASS) developed in this study was equipped with three water sampling cartridges and sensor nodes for in-situ measurements of water quality at different depths.

The system allows rapid sampling from difficult to access water bodies (inaccessible and dangerous water bodies) with relatively low costs and can operate without intense training for practitioners. It lowers operational cost and is useful for monitoring water reservoirs, lakes, rivers, and ponds periodically/ after natural disasters.

Parameters: Temp, EC, pH, DO.

### [Environmental reviews and case studies: bringing unmanned aerial systems closer to the environment](https://www.cambridge.org/core/journals/environmental-practice/article/environmental-reviews-and-case-studies-bringing-unmanned-aerial-systems-closer-to-the-environment/880BBCDB9AF3491A0A779B7B119659A8). 2015 (15)

The spatiotemporal resolution of these datasets will enable policymakers to better measure the impact of policies